{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":8,"n_cols":13,"rows_kept":8,"merged":[[0,0,0,12],[1,0,1,12],[4,0,4,12],[5,0,5,12],[6,0,6,12],[7,0,7,12]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2024年8月质量管理部（检测）全自动洛氏硬度计采购项目                      项目编号：HG JY-G2024115"]
["序号","子项号","资材编码","资材名称","规格描述","技术参数","单位","数量","交货时间","使用部门","含税单价(元)","生产厂家","备注   "]
[1,"A1247000080001",6700400290,"全自动硬度试验机","见 技术规格书","±0.5 %HRC；6工位自动旋转塔台；测试载荷0.2-250kgf;可测HV / HBW / HR ；最大样品高度320mm；自动X-Y轴载物台：最小移动距离1微米、位移精度≤4微米","台","1","2024-10-30","检验检测中心"]
["注：1、投标报价含税，税率13% ；    \n2、生产厂家要求全称填写准确无误 ；                                                                                                               3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2024年8月质量管理部（检测）全自动洛氏硬度计采购项目         项目编号：HG JY-G2024115"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]